

Using the SWTG Client Tool in demo mode (no software for calculation of the results is needed)
==================================================================================================

1. Enter the URL of the TraCIM Server. For the PTB TraCIM Server use https://tracim.ptb.de
   If you are behind a proxy server, enter the relevant settings (i.e. IP address of the proxy, 
   and username/password, if applicable), otherwise leave the fields blank. 

2. Enter your order ID (also called order key) for a FREE TEST. You can get an order key in the 
   TraCIM webshop (https://tracim.ptb.de) after registration. All other fields (i.e. process ID, software name, etc.) 
   can be left blank at this point.

3. Now you can download the test data by clicking the buttom "Request test data". If nothing goes wrong, you will get
   an xml file with the test data and a process ID <ProcessID> (also called process key).
   The test data are also extracted to xml files in GDE format in the subfolder 
   \tracimTestClientData\<ProcessID>
 
4. Check now the box "Demo mode for free test". This has the consequence that with "Load results" the build-in 
   test results for the free test data are loaded. Note that the box is automatically unchecked when new test data are requested or loaded.

5. Before the build-in results are loaded, the field "Software name", "Software version" and "Software vendor" 
   must be filled in. The field "Software revision" ist optional.
   Further a valid MPE must be specified. Allowed are values between 0.001 micrometer and 0.1 micrometer. 
   If the MPE is set to zero, the default value of 0.001 micrometer is used.
   
6. With "Load results" the build-in results are loaded and transformed to xml. 

7. "Submit results" will send the results to the TraCIM server.

8. If nothing goes wrong, a PDF document containing the test report will open. The PDF is also saved to the folder
   \tracimTestClientData\<ProcessID>
   

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%


Using the SWTG Client Tool to perform a TraCIM test:
===================================================================================================================================

1. Enter the URL of the TraCIM Server. For the PTB TraCIM Server enter https://tracim.ptb.de
   If you are behind a proxy server, enter the relevant settings, otherwise leave the fields blank 

2. Enter your order ID (also called order key) for a free or non-free test. You can get an order key in the 
   TraCIM webshop (https://tracim.ptb.de) after registration.  All other fields (i.e. process ID, software name, etc.) 
   can be left blank at this point.

3. Now you can download the test data by clicking the buttom "Request test data". If nothing goes wrong, you will get
   an xml file with the test data and a Process ID <ProcessID> (also called process key).
   The test data are also extracted to xml files in GDE format files in the subfolder 
   \tracimTestClientData\<ProcessID>
   The test data is also saved as xml to the file testData.xml in the same subfolder. This file can 
   be loaded at a later time by clicking the buttom "Load test data".
 
4. Now the results to the given test data must be calculated by your implementation of the gear evaluation algorithm.
   The results must be saved as xml files in GDE format in the same directory 
   \tracimTestClientData\<ProcessID> 
   The format and names of the files containing the results are evident from the example data in 
   \tracimTestClientData\L5A0M73DN5UO3FIQ
                                 
5. Before the calculated results are loaded, the field "Software name", "Software version" and "Software vendor" 
   must be filled in. The field "Software revision" ist optional.
   Further a valid MPE must be specified. Allowed are values between 0.001 micrometer and 0.1 micrometer. 
   If the MPE is set to zero, the default value of 0.001 micrometer is used.
   
6. Make sure the box "Demo Mode" is unchecked. With "Load results" the results from the folder 
   \tracimTestClientData\<ProcessID>
   are loaded and transformed to xml. (The field "Process ID" must contain the appropriate ProcessID.)

7. "Submit results" will send the results to the TraCIM server.  

8. If nothing goes wrong, a PDF document containing the test report will open. The PDF is also saved to the folder
   \tracimTestClientData\<ProcessID>


